\documentclass{report}
\usepackage[utf8]{inputenc}
\usepackage[T1]{fontenc}
\usepackage{textcomp}
\usepackage{geometry}
\geometry{top=15mm, bottom=15mm, left=1cm, right=1cm}
\usepackage[french]{babel}
\usepackage{pslatex}
\usepackage[colorlinks=true,urlcolor=black]{hyperref}
\usepackage{graphicx}
\usepackage{fancyhdr}
\pagestyle{fancy}
\renewcommand{\footrulewidth}{0.4pt}
\fancyfoot[L]{Uubu.fr}
\fancyfoot[R]{lun. févr. 13 10:03:03 CET 2012}
\lfoot{\Large \textit{Uubu.fr}}
\hypersetup{pdfinfo={
Title={openct.conf},
Author={Sylvain Girod},
Creator={Bash script from uubu.fr's format version 1},
Producer={Bash script and PDFLaTeX},
Subject={Fichier de configuration pour openct},
CreationDate={D:20120213100303},
ModDate={D:20120213100303},
Keywords={PKI;sécurité;smartcard}
}}
\begin{document}
 
\begin{center}
{\Huge openct.conf }
\end{center}
\vspace{1cm}
 
\begin{flushleft}
 
{\large Fichier de configuration pour openct}
 
\vspace{10mm}
 
{\ttfamily
debug = 0; \# niveau de debug\\ hotplug = yes; \# Active le mode hotplug\\ \hspace{2mm}\\ \# Path to ifdhandler\\ ifdhandler \{\\ \hspace{2mm}program = /usr/sbin/ifdhandler; \# emplacement de l’ifdhandler\\ \hspace{2mm}force\_poll = 1; \# désactiver si >=2.6.27.14 ou 2.6.28.3\\ \hspace{2mm}user = openctd; \\ \hspace{2mm}groups = \{\\ \hspace{2mm}\hspace{2mm}usb,\\ \hspace{2mm}\};\\ \};\\ \hspace{2mm}\\ ifdproxy \{ \# configuration pour idfproxy\\ \hspace{2mm}server-port = /var/run/openct/.ifdproxy,\\ \hspace{2mm}device-port = :6666;\\ \};\\ \hspace{2mm}\\ \# Liste des lecteurs et leurs options\\ \hspace{2mm}\\ \#reader towitoko \{\\ \# driver = towitoko;\\ \# device = serial :/dev/ttyS0;\\ \#\};\\ \hspace{2mm}\\ \#reader gempc \{\\ \# driver = gempc;\\ \# device = serial :/dev/ttyS0;\\ \#\};\\ \hspace{2mm}\\ \#reader cm4000 \{\\ \# driver = cm4000;\\ \# device = pcmcia :/dev/cmm0;\\ \#\};\\ \hspace{2mm}\\ \#reader cm4040 \{\\ \# driver = ccid;\\ \# device = pcmcia\_block :/dev/cmx0;\\ \#\};\\ \hspace{2mm}\\ \#reader pertosmart1030 \{\\ \# driver = pertosmart1030;\\ \# device = serial :/dev/ttyS0;\\ \#\};\\ \hspace{2mm}\\ \# ID pour Hotplug\\ driver egate \{\\ \hspace{2mm}ids = \{\\ \hspace{2mm}\hspace{2mm}usb:0973/0001,\\ \hspace{2mm}\};\\ \};\\ driver ePass3000 \{\\ \hspace{2mm}ids = \{\\ \hspace{2mm}\hspace{2mm}usb:096e/0401,\\ \hspace{2mm}\};\\ \};\\ driver etoken \{\\ \hspace{2mm}ids = \{\\ \hspace{2mm}\hspace{2mm}usb:0529/050c,\\ \hspace{2mm}\hspace{2mm}usb:0529/0514,\\ \hspace{2mm}\};\\ \};\\ driver etoken64 \{\\ \hspace{2mm}ids = \{\\ \hspace{2mm}\hspace{2mm}usb:0529/0600,\\ \hspace{2mm}\hspace{2mm}usb:0529/0700,\\ \hspace{2mm}\};\\ \};\\ driver eutron \{\\ \hspace{2mm}ids = \{\\ \hspace{2mm}\hspace{2mm}usb:073d/0005,\\ \hspace{2mm}\};\\ \};\\ driver ikey2k \{\\ \hspace{2mm}ids = \{\\ \hspace{2mm}\hspace{2mm}usb:04b9/1202,\\ \hspace{2mm}\};\\ \};\\ driver ikey3k \{\\ \hspace{2mm}ids = \{\\ \hspace{2mm}\hspace{2mm}usb:04b9/1300,\\ \hspace{2mm}\};\\ \};\\ driver starkey \{\\ \hspace{2mm}ids = \{\\ \hspace{2mm}\hspace{2mm}usb:096e/0005,\\ \hspace{2mm}\};\\ \};\\ driver cardman \{\\ \hspace{2mm}ids = \{\\ \# usb:076b/0596, \# OMNIKEY CardMan 2020\\ \# usb:076b/1784, \# OMNIKEY CardMan 6020\\ \# usb:08d4/0009, \# Fujitsu Siemens SCR USB Reader\\ \hspace{2mm}\};\\ \};\\ driver ccid \{\\ \hspace{2mm}ids = \{\\ \hspace{2mm}\hspace{2mm}usb:03f0/1024, \# HP Keyboard with CCID reader\\ \hspace{2mm}\hspace{2mm}usb:046a/0010, \# Cherry smartboard G83-6744\\ \hspace{2mm}\hspace{2mm}usb:04e6/5115,\\ \hspace{2mm}\hspace{2mm}usb:04e6/5116,\\ \hspace{2mm}\hspace{2mm}usb:04e6/5117, \# SCM Micro token size reader\\ \hspace{2mm}\hspace{2mm}usb:04e6/511d, \# SCM Micro SCR3311\\ \hspace{2mm}\hspace{2mm}usb:04e6/E001,\\ \hspace{2mm}\hspace{2mm}usb:04e6/E003,\\ \hspace{2mm}\hspace{2mm}usb:073d/0c00, \# Eutron SimPocket (doesn’t work yet)\\ \hspace{2mm}\hspace{2mm}usb:076b/1021, \# OmniKey CardMan 1021\\ \hspace{2mm}\hspace{2mm}usb:076b/3021,\\ \hspace{2mm}\hspace{2mm}usb:076b/5121,\\ \hspace{2mm}\hspace{2mm}usb:076b/5321, \# OmniKey CardMan 5321\\ \hspace{2mm}\hspace{2mm}usb:076b/6622, \# OmniKey CardMan 6121\\ \hspace{2mm}\hspace{2mm}usb:0783/0003,\\ \hspace{2mm}\hspace{2mm}usb:08e6/3437, \# Gemplus\\ \hspace{2mm}\hspace{2mm}usb:08e6/3438, \# Gemplus GemPC Key SmartCard Reader\\ \hspace{2mm}\hspace{2mm}usb:08e6/4433, \# Gemplus\\ \hspace{2mm}\hspace{2mm}usb:0b97/7762, \# O2 Micro, Inc. Oz776 SmartCard Reader\\ \hspace{2mm}\hspace{2mm}usb:0b97/7772, \# O2 Micro, Inc. Oz776 SmartCard Reader\\ \hspace{2mm}\hspace{2mm}usb:0bf8/1006, \# fujitsu siemens 3.5" drive size reader\\ \hspace{2mm}\hspace{2mm}usb:0dc3/1004, \# Athena Smartcard Solutions, Inc. ASEKey\\ \hspace{2mm}\hspace{2mm}usb:0a89/0030, \# Aktiv Rutoken ECP\\ \hspace{2mm}\};\\ \};\\ driver pertosmart1030 \{\\ \hspace{2mm}ids = \{\\ \hspace{2mm}\hspace{2mm}usb:072f/0001,\\ \hspace{2mm}\hspace{2mm}usb:072f/8009,\\ \hspace{2mm}\};\\ \};\\ driver pertosmart1038 \{\\ \hspace{2mm}ids = \{\\ \hspace{2mm}\hspace{2mm}usb:072f/9000,\\ \hspace{2mm}\hspace{2mm}usb:072f/9006, \# ACS CryptoMate Token\\ \hspace{2mm}\hspace{2mm}usb:072f/9007, \# ACS ACR 100 SIMFlash\\ \hspace{2mm}\hspace{2mm}usb:072f/90d0,\\ \hspace{2mm}\};\\ \};\\ \#driver wbeiuu \{ \# driver not working yet\\ \# ids = \{\\ \# usb:104f/0004,\\ \# \};\\ \#\};\\ \hspace{2mm}\\ \# Tested with USBID 0c4b:0100. These are red readers : one with LCD,\\ \# another one without.\\ driver cyberjack \{\\ \hspace{2mm}ids = \{\\ \hspace{2mm}\hspace{2mm}usb:0c4b/0100,\\ \hspace{2mm}\};\\ \};\\ driver rutoken \{\\ \hspace{2mm}ids = \{\\ \hspace{2mm}\hspace{2mm}usb:0a89/0020, \# Aktiv Rutoken S\\ \hspace{2mm}\hspace{2mm}usb:0a89/0012, \# Aktiv uaToken S\\ \hspace{2mm}\};\\ \};\\
}
\vspace{8mm}
\end{flushleft}
\end{document}
